**How to setup wireless access control of I12**

Product line: AP Model number: I12

This article will guide you how to setup wireless access control of I12 and the steps as below.


**Part 1**: Installation the devices

**Part 2**: Configure your computer

**Part 3**: Login management interface

**Part 4**: Setup wireless access control



1. Power on the AP, and connect your PC to one of the **LAN** ports by a cable, as the following illustration;



1. Right click on **Network Connection Icon** on the system bar, then click on **Open Network and Sharing Center**.


2. Click on **Change adapter settings**.

3. **Right** click on **Local Area Connection**, then choose the **Properties** option.




4. **Double** click on **Internet Protocol Version 4(TCP/IPv4)**.

5. Choose **Use the following IP address** and **Use the following DNS server addresses** and then Set a static IP for local area connection within the following range: **192.168.0.X( 1-253)**, and with the subnet mask: **255.255.255.0** and Default gateway with **192.168.0.254**;



6. Also click on **OK** on the first **Local Connection Properties** window.




1. Launch IE browser, input 192.168.0.254 in the address bar and press **Enter**;
2. Type in the default username and password( **admin** for both) and click **Login**;
3. Then enter this device’s web page;



1. Click **Wireless** item then choose **Access Control** and then setup wireless access control according to the screenshot.

**Mac Address Filter**: Select Allow or Deny from the drop-down list.



1. Now, you have already setup the Access Control, but you cannot access to the Internet without permitted MAC. If you have any problem, please contact our customer service, the email address is [support@tenda.com.cn](mailto:support@tenda.com.cn), thank you.