**FH456--** **How to setup Bandwidth Control**

Note: This article will guide you how to setup speed control and the steps as below.

Step 1: Connect your computer to the LAN port .Power on the FH456.****

You can also use your smartphone to configure the router.

****

Step 2: Open a Web Browser -> Input http://tendawifi.com or 192.168.0.1 in the address bar -> Press Enter

****

Step 3: Go to Bandwidth Control and choose the device you want to control. Set the speed of upload limit and download limit, then click “OK” to save all the settings.

