**How to connect to the network**

****

1. Connect one powerline adapter (such as P3) to any LAN port of your router via an Ethernet cable and plug it into a wall outlet nearby.
2. Plug the wireless extender（PA6） to your chosen place. When both of the PLC LED indicators on the powerline adapter and wireless extender turn solid, a powerline network is established.
3. Connect your wireless devices or computer (with wireless adapter) to the wireless extender（PA6） wirelessly or via an Ethernet cable.
4. The default WiFi name is Tenda\_XXXXXX, which can be found on the rear panel of the extender（PA6）. And there is no default WiFi password.