
**Tenda U3-How to use U3 SoftAP?**




Tenda U3 supports two kinds of working modes: Adapter and SoftAP. SoftAP can transfer your computer’s wired network into wireless signal. Soft-AP is working only when PC could access the internet.

**Note**: Windows 10 system does not support SoftAP. If you want to use SoftAP, please download the third-party sharewares, such as CM Free Wi-Fi, 360 shared Wi-Fi, etc.

Step 1: Install Tenda U3 driver. (Method 1: Insert the CD into the CD-ROM driver; Method 2: Download the driver from the [www.tendacn.com](http://www.tenda.com)) The UI interface as follows appears after the installation means the installation is successful.





Step 2: Click **SoftAP**, then click **Switch**, you can switch to SoftAP.(switching process takes 1-2 minutes)



Step 3: After the success of switch, you can see the default WIIF Name and WIFI Password.



Step 4: To modify the Wi-Fi name or Wi-Fi password, click **Modify**,enter the new Wi-Fi or password, and click **Save**.

****

Step 5: To switch to Adapter, click **Adapter**, then click **Switch**.

