**How to login management interface of I6**

Product line: AP Model number: I6

This article will guide you how to login management interface of I6 and the steps as below.

**Part 1**: Installation the devices

**Part 2**: Configure your computer

**Part 3**: Login management interface



1. Power on the AP, and connect your PC to one of the **LAN** ports by a cable, as the following illustration;



1. Right click on **Network Connection Icon** on the system bar, then click on **Open Network and Sharing Center**.

2. Click on **Change adapter settings**.

3. **Right** click on **Local Area Connection**, then choose the **Properties** option.



4. **Double** click on **Internet Protocol Version 4(TCP/IPv4)**.

5. Choose **Use the following IP address** and **Use the following DNS server addresses** and then Set a static IP for local area connection within the following range: **192.168.0.X( 1-253)**, and with the subnet mask: **255.255.255.0** and Default gateway with **192.168.0.254**;



6. Also click on **OK** on the first **Local Connection Properties** window.



1. Launch IE browser, input 192.168.0.254 in the address bar and press **Enter**;
2. Type in the default username and password( **admin** for both) and click **Login**;
3. Then enter this device’s web page;

**Note**: The above steps shows how to login Management Interface of I6, if you cannot login, please contact our customer service. The email address is support@tenda.com.cn, thank you.