**O3 v2.0--** **How to setup AP Mode**

Note: This article will guide you how to setup AP mode and the steps as below. In this mode, the device creates a wireless network based on the current wired network.


Step 1: Connect the computer to the device

1.1 Open the plastic cover of O3.

1.2 Connect the PoE LAN/WAN port to the PoE injector.


1.3 Power on the O3, the LAN/WAN LED indicator of the O3 lights up.

1.4 Connect your computer to the LAN port of the PoE injector.




Step 2: Enter management interface of O3

2.1 Open a Web Browser -> Input 192.168.2.1 in the address bar -> Press Enter


****

2.2 Typethe default username and password (admin for both defaults) and click “Login”.


****

Step 3: Select AP Mode


3.1 Click “Quick setup”, select “AP”.



3.2 Modify custom local wireless network parameters and click “Next”.



3.3 Click “Save”.



The Current Mode is AP Mode.

