**How to check Rx rate and Tx rate?**

**Step 1**: Open the browser and input plc.tendawifi.com in address bar to login setup page. By default, password is “admin”.



**Step 2**: Choose “Powerline” > “Powerline Device List”.

