**How to login the web interface of Powerline Extender?**

**Step 1**: Use ethernet cable to connect PC with PA6 or connect PA6 WiFi by PC.

**Step 2**: Open bowser and enter **plc.tendawifi.com** in address bar to login the setup page.



**Step 3**: Enter default password “admin” in “Login password” and tap “Login” button.

