**Tenda AC5-How to setup PPTP, L2TP**


Model Number: Tenda AC5

Question Classification: Function Setting


Step 1: Open a browser and type [tendawifi.com](http://tendawifi.com) in Address Bar, tap “Enter”. Input login password and tap “Login”.



Step 2: Tap “VPN”. and choose “PPTP/L2TP Client”.



Step 3: Enter correct VPN information and tap “Connect”.



Step 4: If connect successfully, you can see “Connected” in connection status.