**How to Setup Static IP Connection Mode for AC6**

There are three internet connection mode for the router. This article will guide you how to setup the router for Static IP mode and the steps as below.

Model number: AC6 Question Classification: Internet Settings

**Note**: If you have no idea about what is the internet connection type and the accounts please call your ISP for them.

**Part 1**: Connect the devices

**Part 2**: Configure your computer

**Part 3**: Setup the router

**Part 4**: Check whether you can access internet



Connect the Ethernet cable with the **WAN** port of the router, and then connect your computer with one of the **LAN** ports by a cable.



****

**1** Click on **Network Connection Icon** on the system bar, then click on **Open Network and Sharing Center**.

****

**2** Click on **Change adapter settings**.

****

**3 Right** click on **Local Area Connection**, then choose the **Properties** option.

****

**4 Double** click on **Internet Protocol Version 4(TCP/IPv4)**

****

**5** Choose **Obtain an IP address automatically** and **Obtain DNS server address automatically** and then click **OK**.

****

**6** Also click on **OK** on the first **Local Connection Properties** window.

****

****

**Note：**We need to skip the quick setup to go to advanced settings page to configure if your network connection mode is Static IP.

**1.**Open a browser then type **http://tendawifi.com** in the**address bar**, press **Enter**. And go to the homepage of the router. Then click “**Start**”.



**2.** Click on **Skip** so that we can go to advance to setup the static IP connection mode.



**3.**Setup the wireless name and wireless password. You need to set a login password as well. Then click on **Next.**

****

**Note**: **Wireless password** should be at least **8** characters.

The **Login password** should be 5~32 characters.

1. Click on **Internet Settings**, select the connection type as **Static IP.** Then input the related network info that your ISP gives you. Click **Save.**

****



1. Click on **Internet Status**, if it shows **Connected,** means you can get internet. Enjoy it.



**NOTE:**

When the **Connection Status** Show **Connecting**, please try the steps as below.

1. Click **System Settings**🡪**WAN settings**, you will see a pop-up window.

****

1. In WAN Settings, please choose **Clone MAC Address** in the drop-menu. Then click **Save.**

****