**How to setup the router as PPPOE Internet connection mode**

Model number: FH307

There are three internet connection modes for the router. This article will guide you how to setup the router for PPPOE mode and the steps are as below.

**Note**: if you have no idea about the internet connection type and the accounts please call your ISP for help.

**Part 1**: [Connect these devices](http://www.tendacn.com/en/faq/2486.html%22%20%5Cl%20%224%2C0%2C19%2C0%2C%2CConnect%20the%20devices)

**Part 2**: [Configure your computer](http://www.tendacn.com/en/faq/2486.html%22%20%5Cl%20%22_Hlk371926727)

**Part 3**: [Setup the router](http://www.tendacn.com/en/faq/2486.html%22%20%5Cl%20%224%2C63%2C79%2C0%2C%2CSetup%20the%20router)

**Part 4**: [Check whether you can access internet](http://www.tendacn.com/en/faq/2486.html%22%20%5Cl%20%22_Hlk371926892)



Connect the modem with the **WAN** port of the router, and then connect your computer with one of the **LAN** ports of the router by a cable.



Note: After connection the **SYS** light should be blinking, the **WLAN** light should be on or blinking, the **WAN** light should be on or blinking.



**1** Click **Network Connection Icon** on the system tray, then click **Open Network and Sharing Center**.



**2**Click on **Change adapter settings**.



**3 Right**click **Local Area Connection**, then choose **Properties** option.



**4 Double**click on**Internet Protocol Version 4(TCP/IPv4)**



**5**Choose**Obtain an IP address automatically**and**Obtain DNS server address automatically**and then click**OK**.



**6**Also click **OK** on the first **Local Connection Properties**window

****

****

**1**Open a browser then type **192.168.0.1** in address bar, click **Enter**.



**2** Fill in admin in the **Password** field, click **OK** to login.



**3**Choose the**PPPOE** option, then type the **ISP Username** and **ISP Password** in the correct bars, then set a **2.4G** **Security**as you want, click **OK** to save the settings, then click **Advanced** to login the advanced setting page.



**Note**: the **Security** **Key** should be at least **8** characters.

**4** Click on **Tools**, then click on **Reboot**, and then press the **Reboot The Router** button to reboot the router for refreshing the device info.





Type the User Name and Password as admin then Click on **Advanced**to login the advances setting page, and then check on the **Status.**

If the **Connection** **Status** shows **Connected** that means you can access internet, please check.

