**How to use LED control feature of Powerline Extender?**

**Step 1**: Open the browser and input plc.tendawifi.com in address bar to login setup page. By default, password is “admin”.



**Step 2**: Choose “System” > “LED Control”.



**Note**: If you choose “Schedule”, please follow the instruction to finish the settings and tap “OK” to save the settings.

