**How to check Rx and Tx rate**

**Step 1**: Open bowser and enter plc.tendawifi.com in address bar to login the setup page.



**Step 2**: Choose powerline list. And pay attention to “PLC Device List”. And you can check Tx Rate and Rx Rate.

