## **What to do when your Tenda U2 cannot install the driver automatically?**

# Model: Tenda U2 Problem classification: driver installation

## Phenomenon 1: The computer system does not set the automatic playback function(Control Panel - AutoPlay – Use AutoPlay for all media and devices), the installation tips will not pop up after the insert of NIC, and you need to install manually.

## Open the icon named “computer” or “my computer” or “this computer” on the computer desktop, find the “CD Drive Wireless”, right click it and then select “Open”;

##

## In the list, double-click the “Setup” application to start installing the driver;

##

## When the progress bar go to the end and disappear, and there will be a pop-up dialog box which reminds you that the installation has completed in the bottom right of the computer. Then you can connect to the Internet.

##

##



## Phenomenon 2: The computer can not recognize CD driver. Please refer to the following steps (using Windows 7 as an example):

## Click the “Start” icon on the desktop and select Control Panel;

##

## Click “Uninstall a program”;

##

## Find and uninstall other installed driver-free network card driver, and then reinsert U2, then you can start the installation.