**How to change the SSID and wireless password**

Model number: FH307

If you want to manifest personality and protect your wireless network, you can follow this article to set a personal Wi-Fi name and wireless password.

**Part 1**:[Login the homepage of the router](http://www.tendacn.com/en/faq/2489.html%22%20%5Cl%20%22_Hlk372193340)

**Part 2**: [Change the SSID and wireless password](http://www.tendacn.com/en/faq/2489.html%22%20%5Cl%20%22_Hlk372193369)

**Part 3**: [Reboot the router](http://www.tendacn.com/en/faq/2489.html%22%20%5Cl%20%224%2C93%2C110%2C0%2C%2CReboot%20the%20router)



Open a browser then type **192.168.0.1** in the address bar, click “Enter”.





**1** Fill in ‘admin’ in **Password** fields, click**OK**to login.



**2** Click **Advanced**on the home page to login the advanced setting page.



 **3** Click **Wireless**, then click**Wireless Basic Security**,making sure **Enable Wireless** and **SSID Broadcast** were checked. Also you can change the**Primary SSID** as you want, then click **OK**to save the settings.



**Note**: the **Channel 1, Channel 6** and **Channel 11**are recommended, since there are a little interference.

**4** Click **Wireless**, then click **Security** and choose the **Security mode** as **WPA-PSK**,set a **Security Key**as you want.At last, let the other options as default and hit**OK**to save the settings.





Click **Tools**, and then choose the **Reboot** option on the left of the page, then click **Reboot.**

**The Router**and**OK** to refresh the device info.


     Congratulations!  You can enjoy your wireless network with new Wi-Fi name and new password.

**Note**: 1: Disable the WPS Setting before you change the wifi password.

 2: Security Key should be at least 8 characters.

 3: We recommend AES security mode.

 4: You need to reconnect to the wifi signal after the device reboot.