**How to Setup WPS Function for AC6**

**This document applies to users who need to use WPS function**

Model: Tenda AC6 Question Classification: Function Setup

Step 1: Open a browser on your computer, input [**tendawifi.com**](http://tendawifi.com)in address bar, then press enter key on your keyboard, enter login password of router’s management interface, click “Login”.



Step 2: Click “Wireless Settings”, choose “WPS”.



Step 3: Enable “WPS” function, choose WPS method that you need.

