**How to setup the Black and White list**

This article will guide you how to setup a black and white list and the steps as below

Model Number: F9       Question Classification: Speed Control



The computer can connect to the router via the Internet connection, it can be connected wirelessly to the router if it is a laptop.

Wired Connection:



Wireless Connection:





Open a browser then type **http://tendawifi.com** into the**Address Bar** and then press **Enter**. Typing login password in the homepage of router then click “**Login**”.





Set the blacklist: the device on the blacklist cannot connect to the F9 wireless signal. The other equipment is normal

Method 1: open "**Bandwidth Control**", can make the screen setting for the online device. The diagram below, click on the corresponding equipment behind the "**Internet Access**" column switch button, close to the current equipment shielding, then click "ok" to save.



Method 2: open the "**Advance"** - "**MAC Address Filter**", choose the blacklist, then connect to ban WIFI device's MAC address to fill in in, click "**+**", click "**Ok**", and to save.



**If you need to remove a device from the blacklist, two methods:**

Method 1: remove restriction from "**Bandwidth Control**" - "**blacklist list**" and click "**Ok**";



Method 2: In" **Advance** "-" **blacklist list** "and click" **Ok** "to save.

****

**White list: no other device can connect to the wireless signal except for the white list**

You can add all current online devices, or manually add the device's MAC address.

****