
**How to configure wireless guest network?**

**Step 1**: Open the browser and input plc.tendawifi.com in address bar to login setup page. By default, password is “admin”.



**Step 2**: Choose “Guest Network”, turn on the button.



Note:

User Isolation:

Enable: if the “Enable” option is selected, wireless devices connected to the guest

network cannot communicate with each other.

Disable: if the “Disable” option is selected, wireless devices connected to the guest

network can communicate with each other.