**How to update the firmware of Powerline Extender?**

**Step 1**: Open the browser and input plc.tendawifi.com in address bar to login setup page. By default, password is “admin”.



**Step 2**: Choose “System” > “Firmware Upgrade”.



**Step 3**: You can choose “Online Upgrade” or “Local Upgrade”.



**Note**: If you choose “Local Upgrade”, please download the firmware form Tenda official website. Tap “Select” to upload the firmware from your PC. Please reset the PLC after upgrade is finished.

