
**Tenda U3-How to install driver under MAC System**


**Note**: The currently supported version of the Mac is 10.12, and it can be downwards compatible with other Mac versions.

The specific installation steps are as follows:


1. Download driver on Tenda official website, http://tendacn.com/en/download/detail-3070, the software is a Zip Folder, you can double-click to unzip it.




2. Enter the unzipped file folder, double-click **install.pkg** to install the driver. (Note: **Uninstall.pkg** is used to uninstall the driver)




3.Then the **Welcome** page appears, click **Continue**.




4.Then come into the **Read me** column, click **Continue**.





5.Then come into **Software License Agreement** column, choose your language (English/Traditional Chinese), click **Continue->Agree**, then come into the installation page.







6.Click **Install**, then the login page appears, enter your computer password, click **Install the Software**. You can see the installation progress through the progress bar.







7.Wait for about 1 minute, then click **Restart** when you see installation successful page.



8.After your computer is restarted, you can click on the Wi-Fi icon on the top right side of the screen or click the **system preferences ->network->wlan** to connect Wi-Fi.